Crane Shift Inspection Checklist   Rev 0 · Nov 2026
Visual and functional checks a competent person makes each shift under 29 CFR 1926.1412(d). Use the manufacturer’s manual alongside it.
	Crane make / model
	
	Unit / serial no.
	

	Date
	
	Shift / hour meter
	

	Competent person
	
	Signature
	



	Check
	Source
	OK
	Defect
	N/A
	Notes

	Control mechanisms: no maladjustment interfering with operation
	1412(d)(1)(i)
	☐
	☐
	☐
	

	Control and drive mechanisms: no excessive wear or contamination by lubricant, water or debris
	1412(d)(1)(ii)
	☐
	☐
	☐
	

	Air, hydraulic and other pressurized lines: no deterioration or leaks, especially where they flex
	1412(d)(1)(iii)
	☐
	☐
	☐
	

	Hydraulic system: proper fluid level
	1412(d)(1)(iv)
	☐
	☐
	☐
	

	Hooks and latches: no deformation, cracks, excessive wear or damage
	1412(d)(1)(v)
	☐
	☐
	☐
	

	Wire rope reeving: matches the manufacturer’s specifications
	1412(d)(1)(vi)
	☐
	☐
	☐
	

	Wire rope: no broken wires, kinks, crushing, birdcaging, corrosion or heat damage beyond limits
	1412(d)(1)(vii); 1413(a)
	☐
	☐
	☐
	

	Electrical apparatus: works properly; no excessive deterioration, dirt or moisture
	1412(d)(1)(viii)
	☐
	☐
	☐
	

	Tires (when in use): proper inflation and condition
	1412(d)(1)(ix)
	☐
	☐
	☐
	

	Ground conditions: proper support; no settling under outriggers or crawlers; no standing water
	1412(d)(1)(x)
	☐
	☐
	☐
	

	Crane is level within the manufacturer’s tolerances
	1412(d)(1)(xi)
	☐
	☐
	☐
	

	Operator cab windows: no significant cracks or breaks that block the view
	1412(d)(1)(xii)
	☐
	☐
	☐
	

	Rails, rail stops, rail clamps and supporting surfaces (rail-traveling equipment)
	1412(d)(1)(xiii)
	☐
	☐
	☐
	

	Safety devices and operational aids work properly
	1412(d)(1)(xiv)
	☐
	☐
	☐
	

	Load charts and operating procedures for this configuration are in the cab
	1417(c)(1)
	☐
	☐
	☐
	


Defects found
	Defect
	Safety hazard? Action taken
	Corrected by / date

	
	
	

	
	
	

	
	
	


If the competent person finds a deficiency that is a safety hazard, take the equipment out of service until it is corrected (1926.1412(d)(2)). OSHA does not require the shift inspection to be written down. A monthly inspection must be documented with the items checked, results, the inspector’s name and signature and the date, and kept at least 3 months (1412(e)(3)). A completed copy of this form can serve as that record.
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A blank form for your own program. Filling it in does not qualify, certify or train anyone. Training and qualification are the employer’s responsibility. Check the cited regulation or standard for exact wording.
